#0 $dumpon
$date today $end
$timescale 1 ns $end
$scope module top $end
$var wire 1 0 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/line1_debounced $end
$var wire 1 1 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/line2_debounced $end
$var wire 4 2 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/trigger_line $end
$var wire 2 3 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_trigger_mode $end
$var wire 2 4 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_sourceA_sel $end
$var wire 2 5 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_sourceB_sel $end
$var wire 1 6 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_counter_rst $end
$var wire 32 7 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_counter $end
$var wire 2 8 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_counter_mode $end
$var wire 1 9 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_trigger_out $end
$var wire 1 a ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_sourceA $end
$var wire 1 b ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/encoder_sourceB $end
$var wire 1 c ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/trigger_forward $end
$var wire 1 d ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/trigger_backward $end
$var wire 2 e ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/encoder_sourceA_dly $end
$var wire 2 f ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/encoder_sourceB_dly $end
$var wire 1 10 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/encoder_sourceA_pos $end
$var wire 1 11 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/encoder_sourceA_neg $end
$var wire 1 12 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/encoder_sourceB_neg $end
$var wire 1 13 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_forward0 $end
$var wire 1 14 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_forward1 $end
$var wire 1 15 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_forward2 $end
$var wire 1 16 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_forward3 $end
$var wire 1 17 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_backward0 $end
$var wire 1 18 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_backward1 $end
$var wire 1 19 ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_backward3 $end
$var wire 1 1a ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encoder_control_top_inst/u1_encoder2trigger/trigger_backward2 $end
$var wire 32 1b ins_top_s4/inst_apb3_device/extern_trigger_top_inst/encode_rcounter $end
$upscope $end
$enddefinitions $end
#0
$dumpvars
00
11
b1110 2
b00 3
b00 4
b01 5
06
b00000000000000000010000111001101 7
b00 8
09
0a
1b
0c
0d
b00 e
b11 f
010
011
012
013
014
015
016
017
018
019
01a
b00000000000000000000000000000000 1b
$end
#1021
10
b1111 2
#1022
1a
#1023
b01 e
110
117
#1024
1d
b11 e
010
017
#1025
b00000000000000000010000111001110 7
19
0d
#1026
09
#2047
10
11
b1111 2
b00 3
b00 4
b01 5
06
b00000000000000000010000111001110 7
b00 8
09
1a
1b
0c
0d
b11 e
b11 f
010
011
012
013
014
015
016
017
018
019
01a
b00000000000000000000000000000000 1b
